Filling and placing of geo-textile bags of different sizes and capacity at project site, filling with sand (Dry and minimum 80% Sand must be retained on sieve no 100), sewing one transverse top side after filling sand staking in measurable stakes, marking with synthetic enamel paint during counting and placing in position as per drawing. The total Geo-bag Strip Plan and Progress (source from BWDB) Koyra Horipur Chainge K.M 17.650 to 18.050=400m. CH:16.150 to 16.740 Dumping Length 32m and CH: 16.640 to 17.150 Dumping Length 26m.TBM R.L Taken from Mandir. RL=2.540. Position 741390.965E, 2464006.401N.
